;
;   USBVCOM.INF (for Windows 2000/XP)
;
;   Copyright (c) 2004-2006, DriverCoding Technology Inc.
;
;
[version]
signature="$Windows NT$"
Class=Ports
ClassGuid={4D36E978-E325-11CE-BFC1-08002BE10318}
Provider=%Pro%
DriverVer=06/17/2008,1.0.73.0

[SourceDisksNames]
1=%Pro.Disk%,,,

[SourceDisksFiles]
VCP4USB.sys=1
usbvcom.sys=1

[DestinationDirs]
DefaultDestDir=12
ComPort.NT.Copy=12


[Manufacturer]
%Pro%=Models

[Models]
%DeviceDesc% = ComPort, USB\VID_340d&PID_9066
%DeviceDesc% = ComPort, USB\VID_12d1&PID_3609

[ComPort.NT]
CopyFiles=ComPort.NT.Copy
AddReg=ComPort.NT.AddReg

[ComPort.NT.HW]
AddReg=ComPort.NT.HW.AddReg

[ComPort.NT.HW.AddReg]

[ComPort.NT.Copy]
usbvcom.sys

[ComPort.NT.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,usbvcom.sys
HKR,,EnumPropPages32,,"MsPorts.dll,SerialPortPropPageProvider"


[ComPort.NT.Services]
AddService = usbserial, 0x00000002, Serial_Service_Inst



[Serial_Service_Inst]
DisplayName    = %Serial.SVCDESC%
ServiceType    = 1               ; SERVICE_KERNEL_DRIVER
StartType      = 3               ; SERVICE_SYSTEM_START (this driver may do detection)
ErrorControl   = 1               ; SERVICE_ERROR_IGNORE
ServiceBinary  = %12%\usbvcom.sys
LoadOrderGroup = Base


[Strings]
Pro = "HUAWEI"
Pro.Disk="HUAWEI COM Diskette"
DeviceDesc = "HUAWEI USB COM 1.0"
Serial.SVCDESC   = "HUAWEI COM driver"
